**TEMPOMATIC 5 electronic tap**

Battery-operated

Without stopcocks

Reference: **449106**

Specification description

Deck-mounted electronic basin tap:

Battery-operated with CR123 Lithium 6V batteries.

Reduced stagnation solenoid valve and electronic unit integrated in tap body.

Flow rate pre-set at 3 lpm at 3 bar, from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after the last use).

Active infrared presence detection sensor at the end of the spout optimises detection.

Chrome-plated metal body.

PEX flexible F3/8" with filter.

Fixing reinforced by two stainless steel rods.

Anti-blocking security.

Suitable for people with reduced mobility.

30-year warranty.